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“Please pay attention to copyright note DIN ISO 16016
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"Schutzvermerk nach DIN ISO 16016 beachten”

Z(2:1) Y(2:1)
15,04

5 97 9,02
Fur Version mit Einlegedichtuna: 149 7,32
Schutzart IP40. Um Schutzart IP65 zu erreichen, . cinpress_Gewindebuchsen M3/ . 1,02
muss die beiliegende Dichtung korrekt montiert werden. Press_in threaded insert M3 Y @,
Die Dichtung darf in den Ecken weder gestreckt noch gestaucht werden. u ISTAS
Stof3stelle schrag geschnitten und verklebt, sodaf3 die O I S S Y — [ ﬂ Zeichnungs-Nr. 7
Schnittstellen durch den Federdruck aufeinander gedruckt werden. vl Drawing-No.: 2K 5455.079.01
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For Version with enclosed gasket 4x in_the lid 4\_/\/ —T . .
Protection class IP40. To achieve protection class IP65, Norn Katalogzeichnung/Catalogue drawing
the enclosed gaskef must be mounted correcfly. The gasket must nof be
stretched or compressed in the corners. Ends cut obliquely and glued, 2504628.idw 11 (2:1)
so that the cut ends are pressed fogether by the spring pressure. ol T oo oare o I Az
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